**Important Key Information**

1/ The bath has 2 wastes.

2/ Use shallow waste traps to keep step in threshold to its minimum.

3/ Bath should be fitted rigidly to floor to avoid distortion of doorway when bath is filled..

4/ Do not extend the feet height by using batten runs.

5/Ensure bath foot under doorway is jacked up to maintain bath stability.  ( note only L & P shower baths have outer rigger legs)

6/ Panels can be cut to suit height of bath

7/ As on User Guide it is important the user is advised that the door is always left open when bath is not in use to preserve the seal